**Metal Carving for Jewelry Makers: Supply list**

Round Wire: 1 ft. of 6 or 8 gauge is easiest, but 10 gauge will work as well

Sheet Metal (to make a cuff bracelet): 1” (or larger) by 6” / 16 or 18 gauge (You can use 20 gauge but it won’t be as dramatic)

You can work in silver, copper or brass. It is more important that you learn the technique than which metal you choose.

Please bring your hand tools, flexible shaft supplies, sanding sticks and solder as we will be making a ring and / or bracelet.

A $15 supply fee will be due the day of class.