**“SUGGESTED” SUPPLIES for JEWELRY CLASS**

1. **SAWBLADES:** A package in size 0, and one package in 2/0 or 3/0.
2. **SAWFRAME:** Any style with a 4 or 5 inch throat depth.

**3. DRILL BITS:** Bring sizes 52, 55, 59, 67. (Choose the next lower number if one of the size is not available.)

**4. SANDPAPER AND SANDING STICKS:** In the following grits 240, 320, 400, 600.

Please purchase the "WET/DRY" SILICON CARBIDE type.

**5. FLEXSHAFT ATTACHMENTS** AND THE MANDRELS REQUIRED in order TO USE THEM. This includes sanding discs and their mandrels.

**6. METAL AND WIRE THAT YOU OFTEN USE** in any of the following metals sterling silver, argentium silver, copper or nugold (brass). Basics would include (but not limited to…)

20 gauge sheet metal

Fine Silver Bezel wire (with coordinating stones)

20 gauge round wire (for ear wires) ½ hard sterling silver

10, 12, 14, 16 and 18 gauge round wire dead soft (Whatever sizes you prefer are fine.)

**7. FILES:** Large hand file and needle files.

**8. PLIERS:** flat nose, round nose, chain nose and flush cutters.

**9. TWEEZERS AND SOLDERING PICK**

**10. CENTER PUNCH**

**11. SCRIBE**

**12. ULTRA FINE SHARPIE**

**13. DISH TOWEL and APRON**

**14. CALIPERS and 6” ruler with both inches and millimeters**

**15. DIVIDERS**

**16. MAGIFYING GLASS:** Magni clips, Opti Visor or anything comparable.

**17. SAFETY GOGGLES**

**18. HEARING PROTECTION**

**19. DUST MASK**

**20. RING CLAMP**

**21. SKETCH BOOK AND PENCIL:** to draw or take notes in. Don’t worry about your drawing skills.